**F800R Firmware Instructions**

1. Please use a USB flash drive to copy the firmware to the root directory and the U disk needs to be in FAT32 format. At the same time, only one firmware (bin format) can exist in the root directory.
2. Insert the USB flash drive into the USB port of the light, and turn on the light. Wait for the upgrade progress bar to complete.
3. To check the version number: Go to the menu and check the INFO.
4. Version Instructions:

|  |  |  |
| --- | --- | --- |
| **Version** | **What’s new** | **Date** |
| V1.05 | Optimized known issues | 2025-06-07 |
| V1.04 | Resolved the color gel issue | 2024-09-30 |

**Note: For more details, please download the newest instruction manual on the official website:**

**www.knowled.com.**